
#Navigation > Applications > IVR > Add IVR 

- Name 
- Description 
- Announcement (Initial call recording) 
- Enable Direct Dial (Y/N) .  
    - If Enabled, Configured through #Applications > Directory  
- Timeout 
    - Retries 
    - Recording 
    - Append announcment  
- Invalid Retries 
    - Invalid Recording 
    - Invalid Destination  
    - Append Announcement to invalid 
        - After playing the Invalid retry recording, the system will replay the main IVR announcement    
- IVR Entries 
    - Mapping of entries     
- Submit    
- Apply Config 

Testing 
#Navigaiton > Connectivity > Inbound Routes > Edit 

- Set Destination     
- Apply Config